**DEPARTMENT OF INFORMATION TECHNOLOGY FACULTY OF ENGINEERING & TECHNOLOGY**

###### **IoT PROJECT REPORT**

###### **SUBJECT TITLE : INTERNET OF THINGS**

**SUBJECT CODE: 15IT422E**

**SUBMITTED TO: Prof Kayalvizhi Jayavel**

**HOME AUTOMATION SYSTEM**

HARIHARAN S

RA1611008010115

**Department of Information Technology**



**SRM University, SRM Nagar, Kattankulathur-603203 Kanchipuram District, Tamil Nadu**

LINKS TO GITHUB AND YOUTUBE:

YouTube:

<https://youtu.be/k1RowOjPz24>

Github:

https://github.com/09hari

**ACKNOWLEDGEMENT**

I would like to express my sincere gratitude to our IoT Professor Mrs Kayalvizhi Jayavel for being out there at every step of my course and guiding us all along the way to be capable of moulding our ideas into smart projects.

I would also like to thank my parents, without whom I wouldn’t be able to anything in any regard.

**ABSTRACT**

Home automation system achieved great popularity in the last decades and it increases the comfort and quality of life. In this paper an overview of current and emerging home automation systems is discussed. Nowadays most home automation systems consist of a smartphone and microcontroller. A smart phone application is used to control and monitor the home appliances using different type of communication techniques. In this paper the working principle of different type of wireless communication techniques such as ZigBee, Wi-Fi, Bluetooth, EnOcean and GSM are studied and their features are compared with each other so the users can choose their own choice of technology to build home automation system. Moreover in this research work the survey of different home automation systems is discussed and their advantages and drawbacks are also highlighted.

**HARDWARE REQUIRED:**

* NodeMCU ESP8266
* Bread Board
* Female-Female Jumper wires
* 2-Channel Relay

**SOFTWARE REQUIRED :**

* Arduino IDE.
* ESP8266 library.
* Adafruit MQTT Library.

**MISCELLANEOUS :**

* Wifi Internet Connection
* Soldering tool
* Soldering wires

**TOTAL COST OF COMPONENTS :- RS.1800 - RS.2000.**

**SYSTEM OVERVIEW**

The main component of the setup is the Nodemcu ESP8266 module. All the other hardware components are connected to the Nodemcu. The board is programmed in Arduino IDE and uses the ESP8266, Adafruit MQTT libraries. These libraries have been added to the Arduino IDE. The MPU6050 module with gyroscope and accelerometer is directly connected to the Nodemcu using a micro USB cable.

**Programming NodeMCU and setting up Adafruit Dashboard :**

* Import Adafruit Library to the Arduino IDE
* Fill your Adafruit token, ssid, and wifi password to the code.
* Upload home automation code to your NodeMCU
* Setup your Adafruit dashboard, add a custom widget, choose two state widget and give it name.

**CODE**

**#include <ESP8266WiFi.h>**

**#include "Adafruit\_MQTT.h"**

**#include "Adafruit\_MQTT\_Client.h"**

**/\*\*\*\*\*\*\*\*\* WiFi Access Point \*\*\*\*\*\*\*\*\*\*\*/**

**#define WLAN\_SSID "Incubation"**

**#define WLAN\_PASS "SRMIPcenter"**

**/\*\*\*\*\*\*\*\*\* Adafruit.io Setup \*\*\*\*\*\*\*\*\*\*\*/**

**#define AIO\_SERVER "io.adafruit.com"**

**#define AIO\_SERVERPORT 1883 // use 8883 for SSL**

**#define AIO\_USERNAME "Dymatize"**

**#define AIO\_KEY "9debf6a3fa834e84bf3aa573eb5948eb"**

**/\*\*\*\* Global State (you don't need to change this!) \*\*\*\*\*\*/**

**// Create an ESP8266 WiFiClient class to connect to the MQTT server.**

**WiFiClient client;**

**// or... use WiFiFlientSecure for SSL**

**//WiFiClientSecure client;**

**// Setup the MQTT client class by passing in the WiFi client and MQTT server and login details.**

**Adafruit\_MQTT\_Client mqtt(&client, AIO\_SERVER, AIO\_SERVERPORT, AIO\_USERNAME, AIO\_KEY);**

**/\*\*\*\*\*\*\*\*\*\* Feeds \*\*\*\*\*\*\*\*\*\*\*\*\*/**

**// Setup feeds for publishing.**

**// Notice MQTT paths for AIO follow the form: <username>/feeds/<feedname>**

**// Setup feeds subscribing to changes.**

**Adafruit\_MQTT\_Subscribe LED = Adafruit\_MQTT\_Subscribe(&mqtt, AIO\_USERNAME "/feeds/light");**

**/\*\*\*\*\*\*\*\*\* Sketch Code \*\*\*\*\*\*\*\*\*\*\*\*/**

**// Bug workaround for Arduino 1.6.6, it seems to need a function declaration**

**// for some reason (only affects ESP8266, likely an arduino-builder bug).**

**void MQTT\_connect();**

**void setup() {**

**Serial.begin(115200);**

**delay(10);**

**pinMode(D3,OUTPUT);**

**// Connect to WiFi access point.**

**Serial.println(); Serial.println();**

**Serial.print("Connecting to ");**

**Serial.println(WLAN\_SSID);**

**WiFi.begin(WLAN\_SSID, WLAN\_PASS);**

**while (WiFi.status() != WL\_CONNECTED) {**

**delay(500);**

**Serial.print(".");**

**}**

**Serial.println();**

**Serial.println("WiFi connected");**

**Serial.println("IP address: "); Serial.println(WiFi.localIP());**

**// Setup MQTT subscription**

**mqtt.subscribe(&LED);**

**}**

**uint32\_t x=0;**

**void loop() {**

**MQTT\_connect();**

**Adafruit\_MQTT\_Subscribe \*subscription;**

**while ((subscription = mqtt.readSubscription(5000))) {**

**if (subscription == &LED) {**

**Serial.println((char \*)LED.lastread);**

**int state=atoi((char\*)LED.lastread);**

**digitalWrite(D3,state);**

**}**

**}**

**// Now we can publish stuff!**

**// ping the server to keep the mqtt connection alive**

**// NOT required if you are publishing once every KEEPALIVE seconds**

**/\***

**if(! mqtt.ping()) {**

**mqtt.disconnect();**

**}**

**\*/**

**}**

**// Function to connect and reconnect as necessary to the MQTT server.**

**// Should be called in the loop function and it will take care if connecting.**

**void MQTT\_connect() {**

**int8\_t ret;**

**// Stop if already connected.**

**if (mqtt.connected()) {**

**return;**

**}**

**Serial.print("Connecting to MQTT... ");**

**uint8\_t retries = 3;**

**while ((ret = mqtt.connect()) != 0) { // connect will return 0 for connected**

**Serial.println(mqtt.connectErrorString(ret));**

**Serial.println("Retrying MQTT connection in 5 seconds...");**

**mqtt.disconnect();**

**delay(5000); // wait 5 seconds**

**retries--;**

**if (retries == 0) {**

**// basically die and wait for WDT to reset me**

**while (1);**

**}**

**}**

**Serial.println("MQTT Connected!");**

**}**

**Adafruit Dashboard, Widgets and Triggers :**

We give our WiFi SSID and password inside the code before compiling and uploading it to the Nodemcu. Also in order to connect to the Adafruit database, we give the Adafruit username, Adafruit password and Adafruit client ID so that it can connect via MQTT.

**Result :**

Home Automation using ESP8266 NodeMCU has been successfully developed and implemented.

